.. _ctrl-channel:

**************
Management API
**************

A classic approach to daemon configuration assumes that the server's
configuration is stored in configuration files and, when the
configuration is changed, the daemon is restarted. This approach has the
significant disadvantage of introducing periods of downtime when client
traffic is not handled. Another risk is that if the new configuration is
invalid for any reason, the server may refuse to start, which will
further extend the downtime period until the issue is resolved.

To avoid such problems, the DHCPv4, DHCPv6, and D2 servers in Kea include
support for a mechanism that allows online reconfiguration without
requiring server shutdown. Both servers can be instructed to open
control sockets, which is a communications channel. The server is able
to receive commands on that channel, act on them, and report back
status.

The DHCPv4, DHCPv6, and D2 servers receive commands over the UNIX domain
sockets. For details on how to configure these sockets, see
:ref:`dhcp4-unix-ctrl-channel`, :ref:`dhcp6-unix-ctrl-channel` and
:ref:`d2-unix-ctrl-channel`. While
it is possible to control the servers directly using UNIX domain sockets,
that requires that the controlling client be running on the same machine
as the server. SSH is usually used to connect remotely to the controlled
machine.

Network administrators usually prefer using some form of a RESTful API
to control the servers, rather than using UNIX domain sockets directly.
Therefore, Kea includes a component called the Control Agent (CA), which
exposes a RESTful API to the controlling clients and can forward
commands to the respective Kea services over the UNIX domain sockets.
The CA configuration is described in
:ref:`agent-configuration`.

The HTTP requests received by the CA contain the control commands
encapsulated within HTTP requests. Simply speaking, the CA is
responsible for stripping the HTTP layer from the received commands and
forwarding the commands in a JSON format over the UNIX domain sockets to
the respective services. Because the CA receives commands for all
services, it requires additional "forwarding" information to be included
in the client's messages. This forwarding information is carried within
the ``service`` parameter of the received command. If the ``service``
parameter is not included, or if the parameter is a blank list, the CA
assumes that the control command is targeted at the CA itself and
attempts to respond.

Control connections over both HTTP and UNIX domain sockets are guarded
with timeouts. The timeout value is set to 10 seconds and is not
configurable.

This API can be used by external tools to manage and monitor Kea operation.
An example of such a monitoring tool is ISC's Stork. For details, see
:ref:`stork`.

.. _ctrl-channel-syntax:

Data Syntax
===========

Communication over the control channel is conducted using JSON
structures. If configured, Kea opens a socket and listens for
incoming connections. A process connecting to this socket is expected to
send JSON commands structured as follows:

::

   {
       "command": "foo",
       "service": [ "dhcp4" ],
       "arguments": {
           "param1": "value1",
           "param2": "value2",
           ...
       }
   }

The same command sent over the RESTful interface to the CA has the
following structure:

::

       POST / HTTP/1.1\r\n
       Content-Type: application/json\r\n
       Content-Length: 147\r\n\r\n
       {
           "command": "foo",
           "service": [ "dhcp4" ],
           "arguments": {
               "param1": "value1",
               "param2": "value2",
               ...
           }
       }

The ``command`` parameter contains the name of the command to execute and it
is mandatory.
The ``arguments`` map contains the parameters required to carry out the
given command. The exact content and format of the map are command-specific.

The ``service`` list contains the servers at which the control command is
targeted. In the example above, the control command is targeted at the
DHCPv4 server. In most cases, the CA simply forwards this command to
the DHCPv4 server for processing via a UNIX domain socket. Sometimes,
the command including a service value may also be processed by the CA,
if the CA is running a hook library which handles such a command for
the given server. As an example, the hook library loaded by the CA may
perform some operations on the database, such as adding host
reservations, modifying leases, etc. An advantage of performing
DHCPv4-specific administrative operations in the CA, rather than
forwarding it to the DHCPv4 server, is the ability to perform these
operations without disrupting the DHCPv4 service, since the DHCPv4
server does not have to stop processing DHCP messages to apply changes to
the database. Nevertheless, these situations are rather rare; in
most cases, when the ``service`` parameter contains a name of the
service, the commands are simply forwarded by the CA. The forwarded
command includes the ``service`` parameter, but this parameter is ignored
by the receiving server. This parameter is only meaningful to the CA.

If the command received by the CA does not include a ``service``
parameter or this list is empty, the CA simply processes this message on
its own. For example, a :isccmd:`config-get` command which includes no service
parameter returns the Control Agent's own configuration. The :isccmd:`config-get`
command with a service value "dhcp4" is forwarded to the DHCPv4 server and
returns the DHCPv4 server's configuration.

The following list shows the mapping of the values carried within the
``service`` parameter to the servers to which the commands are
forwarded:

-  ``dhcp4`` - the command is forwarded to the :iscman:`kea-dhcp4` server.

-  ``dhcp6`` - the command is forwarded to the :iscman:`kea-dhcp6` server.

-  ``d2`` - the command is forwarded to the :iscman:`kea-dhcp-ddns` server.

The server processing the incoming command sends a response of the
form:

::

   {
       "result": 0, // 0|1|2|3|4
       "text": "textual description",
       "arguments": {
           "argument1": "value1",
           "argument2": "value2",
           ...
       }
   }

The ``result`` value is a status code indicating a result of the command. The
following general status codes are currently supported:

-  ``0`` - the command has been processed successfully.
-  ``1`` - a general error or failure has occurred during the command processing.
-  ``2`` - the specified command is unsupported by the server receiving it.
-  ``3`` - the requested operation has been completed but the requested
   resource was not found. This status code is returned when a command
   returns no resources or affects no resources.
-  ``4`` - the well-formed command has been processed but the requested
   changes could not be applied, because they were in conflict with the
   server state or its notion of the configuration.

For example, a well-formed command that requests a subnet that exists
in a server's configuration returns the result 0. If the server encounters
an error condition, it returns 1. If the command asks for an IPv6 subnet,
but was sent to a DHCPv4 server, it returns 2. If the query asks for a
subnet with ``subnet-id`` that has matches, the result is 3.
If the command attempts to update a lease but the specified ``subnet-id``
does not match the identifier in the server's configuration, the result
is 4.

Hook libraries can sometimes return additional status codes specific
to their use cases.

The ``text`` field typically appears when the result is non-zero and
contains a description of the error encountered, but it often also
appears for successful outcomes. The exact text is command-specific, but
in general uses plain English to describe the outcome of the command.
The ``arguments`` map contains additional data values returned by the server
which are specific to the command issued. The map may be present, but that
depends on the specific command.

.. note::

   Since Kea 1.9.7, it is possible to put comments in commands as
   in the configuration file. For instance:

::

   {
       "command": "foo",
       // service is a list
       "service": [ "dhcp4" ],
       # command arguments are here.
       "arguments": {
           "param1": "value1",
           ...
           /*
           "param2": "value2",
           ...
           */
       }
   }

.. note::

   Since Kea 2.7.5 it is possible to specify extra HTTP headers which
   are added to HTTP responses. Each header is specified by its name
   and value with optionally a user context. For instance:

::

   {
       "http-headers": [
           {
               "name": "Strict-Transport-Security",
               "value": "max-age=31536000"
           }
        ],
    ...
    }

adds a HSTS header declaring that HTTPS (vs HTTP) must be used for one year.

.. _ctrl-channel-control-agent-command-response-format:

Control Agent Command Response Format
=====================================

When sending commands via the Control Agent, it is possible to specify
multiple services at which the command is targeted. CA forwards this
command to each service individually. Thus, the CA response to the
controlling client is always wrapped in an array (JSON list) of
individual responses.  For example, the response for a command sent
to one service would be structured as follows:

::

    [
        {
            "result": 0, // 0|1|2|3|4
            "text": "textual description",
            "arguments": {
                "argument1": "value1",
                "argument2": "value2",
                ...
            }
        }
    ]


If the command is sent to more than one service, the array would
contain responses from each service, in the order they were requested:

::

    [
        {
            "result": 0, // 0|1|2|3|4
            "text": "textual description",
            "arguments": {
                "argument1": "value1",
                "argument2": "value2",
                ...
            }
        },
        {
            "result": 0, // 0|1|2|3|4
            "text": "textual description",
            "arguments": {
                "argument1": "value1",
                "argument2": "value2",
                ...
            }
        },
        ...
    ]

An exception to this are authentication or authorization errors which cause CA
to reject the command entirely.  The response to such an error is formatted
as a single entry (JSON map) as follows:

::

    {
        "result": 403,
        "text": "Forbidden"
    }


These types of errors are possible on systems configured for either basic
authentication or agents that load :ischooklib:`libdhcp_rbac.so`.

.. _ctrl-channel-client:

Using the Control Channel
=========================

The easiest way to start interacting with the control API is to use
common UNIX/Linux tools such as ``socat`` and ``curl``.

In order to control the given Kea service via a UNIX domain socket, use
``socat`` in interactive mode as follows:

.. code-block:: console

   $ socat UNIX:/path/to/the/kea/socket -

or in batch mode, include the "ignoreeof" option as shown below to
ensure ``socat`` waits long enough for the server to respond:

.. code-block:: console

   $ echo "{ some command...}" | socat UNIX:/path/to/the/kea/socket -,ignoreeof

where ``/path/to/the/kea/socket`` is the path specified in the
``Dhcp4/control-socket/socket-name`` parameter in the Kea configuration
file. Text passed to ``socat`` is sent to Kea and the responses received
from Kea are printed to standard output. This approach communicates with
the specific server directly and bypasses the Control Agent.

It is also easy to open a UNIX socket programmatically. An example of a
simple client written in C is available in the Kea Developer's Guide, in
the Control Channel Overview chapter, in the
`Using Control Channel <https://reports.kea.isc.org/dev_guide/d2/d96/ctrlSocket.html#ctrlSocketClient>`__
section.

To use Kea's RESTful API with ``curl``, use the following:

.. code-block:: console

   $ curl -X POST -H "Content-Type: application/json" -d '{ "command": "config-get", "service": [ "dhcp4" ] }' http://ca.example.org:8000/

This assumes that the Control Agent is running on host
``ca.example.org`` and is running the RESTful service on port 8000.

.. _commands-common:

Commands Supported by Both the DHCPv4 and DHCPv6 Servers
========================================================

.. isccmd:: build-report
.. _command-build-report:

The ``build-report`` Command
----------------------------

The :isccmd:`build-report` command returns on the control channel what the
command line ``-W`` argument displays, i.e. the embedded content of the
``config.report`` file. This command does not take any parameters.

::

   {
       "command": "build-report"
   }

.. isccmd:: config-get
.. _command-config-get:

The ``config-get`` Command
--------------------------

The :isccmd:`config-get` command retrieves the current configuration used by the
server. This command does not take any parameters. The configuration
returned is roughly equal to the configuration that was loaded using the
``-c`` command-line option during server start-up, or was later set using the
:isccmd:`config-set` command. However, there may be certain differences, as
comments are not retained. If the original configuration used file
inclusion, the returned configuration includes all parameters from
all included files. In Kea 2.4.0 and later, the successful response also
contains a SHA-256 digest that can be used to easily determine whether a
configuration has changed.

.. warning::

   The returned configuration is not redacted, i.e. it
   contains database passwords in plain text, if those were specified in the
   original configuration. Care should be taken not to expose the command
   channel to unprivileged users.

An example command invocation looks like this:

::

   {
       "command": "config-get"
   }

.. isccmd:: config-hash-get
.. _command-config-hash-get:

The ``config-hash-get`` Command
-------------------------------

The ``config-hash-get`` command retrieves the SHA-256 hash of the current
configuration used by the server. This command does not take any parameters.
The returned hash can be used to detect configuration changes.

An example command invocation looks like this:

::

   {
       "command": "config-hash-get"
   }

And the server's response:

::

   {
       "result": 0,
       "arguments": {
           "hash": "5C3C90EF7035249E2FF74D003C19F34EE0B83A3D329E741B52B2EF95A2C9CC5C"
        }
    }

In Kea 2.4.0 and later, ``config-set`` and ``config-get`` also return the SHA-256 hash
of the new or current configuration. This may be used to determine whether a configuration
has changed.

.. isccmd:: config-reload
.. _command-config-reload:

The ``config-reload`` Command
-----------------------------

The :isccmd:`config-reload` command instructs Kea to load again the
configuration file that was used previously. This operation is useful if
the configuration file has been changed by some external source; for
example, a system administrator can tweak the configuration file and use this
command to force Kea to pick up the changes.

Care should be taken when using this in conjunction with the :isccmd:`config-set` command. Kea
remembers the location of the configuration file it was started with,
and this configuration can be significantly changed using the :isccmd:`config-set`
command. When :isccmd:`config-reload` is issued after :isccmd:`config-set`, Kea attempts
to reload its original configuration from the file, possibly losing all
changes introduced using :isccmd:`config-set` or other commands.

The :isccmd:`config-reload` command does not take any parameters. An example command
invocation looks like this:

::

   {
       "command": "config-reload"
   }

If the configuration file is incorrect, reloading it can raise an error
which leaves the server in an unusable state. See :ref:`command-config-set`
to learn how to recover from a non-working server.

.. isccmd:: config-test
.. _command-config-test:

The ``config-test`` Command
---------------------------

The :isccmd:`config-test` command instructs the server to check whether the new
configuration supplied in the command's arguments can be loaded. The
supplied configuration is expected to be the full configuration for the
target server, along with an optional logger configuration. The configuration
is sanity-checked to the extent possible without the server actually
attempting to load it; it is possible for a configuration which successfully
passes this command to still fail in the :isccmd:`config-set` command or at launch
time. The structure of the command is as follows:

::

   {
       "command": "config-test",
       "arguments":  {
           "<server>": {
           }
       }
   }

where <server> is the configuration element name for a given server, such
as "Dhcp4" or "Dhcp6". For example:

::

   {
       "command": "config-test",
       "arguments":  {
           "Dhcp6": {
               ...
           }
       }
   }

The server's response contains a numeric code, ``result`` (0 for
success, non-zero on failure), and a string, ``text``, describing the
outcome:

::

       {"result": 0, "text": "Configuration seems sane..." }

       or

       {"result": 1, "text": "unsupported parameter: BOGUS (<string>:16:26)" }

.. isccmd:: config-write
.. _command-config-write:

The ``config-write`` Command
----------------------------

The :isccmd:`config-write` command instructs the Kea server to write its current
configuration to a file on disk. It takes one optional argument, called
"filename", that specifies the name of the file to write the
configuration to. If not specified, the name used when starting Kea
(passed as a ``-c`` argument) is used. If a relative path is specified,
Kea writes its files only in the directory where it is running.

An example command invocation looks like this:

::

   {
       "command": "config-write",
       "arguments": {
           "filename": "config-modified-2017-03-15.json"
       }
   }

.. note::

    As of Kea 2.7.9, the config file file may only be written to the same
    directory as the config file used when starting Kea (passed as a ``-c``
    argument).

.. isccmd:: leases-reclaim
.. _command-leases-reclaim:

The ``leases-reclaim`` Command
------------------------------

The :isccmd:`leases-reclaim` command instructs the server to reclaim all expired
leases immediately. The command has the following JSON syntax:

::

   {
       "command": "leases-reclaim",
       "arguments": {
           "remove": true
       }
   }

The ``remove`` boolean parameter is mandatory and indicates whether the
reclaimed leases should be removed from the lease database (if ``true``), or
left in the ``expired-reclaimed`` state (if ``false``). The latter facilitates
lease affinity, i.e. the ability to re-assign an expired lease to a
returning client that previously used that lease. See :ref:`lease-affinity`
for details. Also, see :ref:`lease-reclamation` for general
information about the processing of expired leases (lease reclamation).

.. isccmd:: list-commands
.. _command-list-commands:

The ``list-commands`` Command
-----------------------------

The :isccmd:`list-commands` command retrieves a list of all commands supported
by the server. It does not take any arguments. An example command may
look like this:

::

   {
       "command": "list-commands",
       "arguments": { }
   }

The server responds with a list of all supported commands. The arguments
element is a list of strings, each of which conveys one supported
command.

.. isccmd:: config-set
.. _command-config-set:

The ``config-set`` Command
--------------------------

The :isccmd:`config-set` command instructs the server to replace its current
configuration with the new configuration supplied in the command's
arguments. The supplied configuration is expected to be the full
configuration for the target server, along with an optional logger
configuration. While optional, the logger configuration is highly
recommended, as without it the server reverts to its default logging
configuration. The structure of the command is as follows:

::

   {
       "command": "config-set",
       "arguments":  {
           "<server>": {
           }
       }
   }

where <server> is the configuration element name for a given server, such
as "Dhcp4" or "Dhcp6". For example:

::

   {
       "command": "config-set",
       "arguments":  {
           "Dhcp6": {
               ...
           }
       }
   }

If the new configuration proves to be invalid, the server retains its
current configuration; however, in some cases a fatal error message is logged
indicating that the server is no longer providing any service: a working
configuration must be loaded as soon as possible. If the control channel
is dead, the configuration file can still be reloaded using the ``SIGHUP``
signal. If that is unsuccessful, restart the server.

Please note that the new configuration is
retained in memory only; if the server is restarted or a configuration
reload is triggered via a signal, the server uses the configuration
stored in its configuration file. The server's response contains a
numeric code, ``result`` (0 for success, non-zero on failure), and a
string, ``text``, describing the outcome:

::

       {"result": 0, "text": "Configuration successful." }

       or

       {"result": 1, "text": "unsupported parameter: BOGUS (<string>:16:26)" }

In Kea 2.4.0 and later, the successful response from a DHCPv4, DHCPv6, or DHCP-DDNS daemon
also contains a SHA-256 digest of the newly set configuration. The digest can be used to easily
determine whether a configuration has changed.

.. isccmd:: shutdown
.. _command-shutdown:

The ``shutdown`` Command
------------------------

The :isccmd:`shutdown` command instructs the server to initiate its shutdown
procedure; it is the equivalent of sending a ``SIGTERM`` signal to the
process. This command does not take any arguments. An example command
may look like this:

::

   {
       "command": "shutdown",
       "arguments": {
           "exit-value": 3
       }
   }

The server responds with a confirmation that the shutdown procedure has
been initiated.  The optional parameter, ``exit-value``, specifies the
numeric value with which the server process exits to the system.
The default value is zero.

The DDNS daemon supports an extra parameter, ``type``, which controls the way
the process cleans up on exit. The supported shutdown types are:

 -  "normal" - stops the queue manager and finishes all current transactions
    before exiting. This is the default.

 -  "drain_first" - stops the queue manager but continues processing requests
    from the queue until it is empty.

 -  "now" - exits immediately.

An example command may look like this:

::

   {
       "command": "shutdown",
       "arguments": {
           "exit-value": 3,
           "type": "drain_first"
       }
   }

.. isccmd:: dhcp-disable
.. _command-dhcp-disable:

The ``dhcp-disable`` Command
----------------------------

The :isccmd:`dhcp-disable` command globally disables the DHCP service. The
server continues to operate, but it drops all received DHCP messages.
This command is useful when the server's maintenance requires that the
server temporarily stop allocating new leases and renew existing leases.
It is also useful in failover-like configurations during a
synchronization of the lease databases at startup, or recovery after a
failure. The optional parameter ``max-period`` specifies the time in
seconds after which the DHCP service should be automatically re-enabled,
if the :isccmd:`dhcp-enable` command is not sent before this time elapses.

Since Kea 1.9.4, there is an additional ``origin`` parameter that specifies the
command source. A server administrator should typically omit this parameter
because the default value "user" indicates that the administrator sent the
command. In Kea 2.5.5 through 2.5.7, this parameter was also used in communication
between the HA partners to specify the identifier of an HA service sending the command
in a numeric format. However, due to compatibility issues with older
Kea versions that did not properly parse numeric values, it was necessary
to introduce the new parameter, ``origin-id``, in Kea 2.5.8.

It holds a numeric value representing the origin of the command. The same value
can still be passed using the ``origin`` parameter, but it can cause the
aforementioned compatibility issues between HA partners running different
Kea versions; if both are used, ``origin-id`` takes precedence. New Kea versions
favor using ``origin-id`` in communication between the HA partners, but
overall, it is recommended that both parameters be
omitted and the default value used.

The following codes represent the supported origins in numeric format:

 -  ``1`` - a user command; the same as specifying ``"origin": "user"``.
 -  ``2000``, ``2001``, ``2002``, etc. - origins specified by HA partners where
    the increments above ``2000`` are distinct HA service identifiers used when
    the partners have many relationships.

In the following example:

::

   {
       "command": "dhcp-disable",
       "arguments": {
           "max-period": 20,
           "origin-id": 2002,
           "origin": "user"
       }
   }

the effective origin is ``2002``, which indicates it is an HA partner
sending the command for the service with ID of ``2``. The ``origin``
parameter will be ignored in this case.

.. isccmd:: dhcp-enable
.. _command-dhcp-enable:

The ``dhcp-enable`` Command
---------------------------

The :isccmd:`dhcp-enable` command globally enables the DHCP service.

Since Kea 1.9.4, there is an additional ``origin`` parameter that specifies the
command source. A server administrator should typically omit this parameter
because the default value "user" indicates that the administrator sent the
command. In Kea 2.5.5 through 2.5.7, this parameter was also used in communication
between the HA partners to specify the identifier of an HA service sending the command
in a numeric format. However, due to compatibility issues with older
Kea versions that did not properly parse numeric values, it was necessary
to introduce the new parameter, ``origin-id``, in Kea 2.5.8.

It holds a numeric value representing the origin of the command. The same value
can still be passed using the ``origin`` parameter, but it can cause the
aforementioned compatibility issues between HA partners running different
Kea versions.; if both are used, ``origin-id`` takes precedence. New Kea versions
favor using ``origin-id`` in communication between the HA partners, but
overall, it is recommended that both

The following codes represent the supported origins in numeric format:

 -  ``1`` - a user command; the same as specifying ``"origin": "user"``.
 -  ``2000``, ``2001``, ``2002``, etc. - origins specified by HA partners where
    the increments above ``2000`` are distinct HA service identifiers used when
    the partners have many relationships.

In the following example:

::

   {
       "command": "dhcp-enable",
       "arguments": {
           "origin-id": 2002,
           "origin": "user"
       }
   }

the effective origin is ``2002``, which indicates it is an HA partner
sending the command for the service with ID of ``2``. The ``origin``
parameter will be ignored in this case.


.. isccmd:: status-get
.. _command-status-get:

The ``status-get`` Command
--------------------------

The :isccmd:`status-get` command returns the server's runtime information:

 - ``pid``: the process ID.

 - ``uptime``: the number of seconds since the start of the server.

 - ``reload``: the number of seconds since the last configuration (re)load.

 - ``high-availability``: HA-specific status information about the DHCP servers
   configured to use the HA hook library:

     * ``local``: the state, the role (primary,
       secondary, ...), and the scopes (i.e. what the server is actually
       processing) of the local server.

     * ``remote``: the remote server's last known state, its served
       HA scopes, and the role of the remote server in the HA relationship.

 - ``multi-threading-enabled``: a flag indicating whether multi-threading is enabled.

 - ``thread-pool-size``: the number of DHCP service threads.

 - ``packet-queue-size``: the maximum size of the packet queue. There is one queue,
   regardless of the number of running threads.

 - ``packet-queue-statistics``: the average queue size for the last 10, 100, and 1000
   packets, using an approach similar to the UNIX ``top`` command.
   The average queue size for the last 10 packets can be considered an
   instantaneous value, while the average for the last 1000 packets shows
   a longer-term trend.

The ``high-availability`` information is returned only when the command is
sent to the DHCP servers in an HA setup. This parameter is
never returned when the :isccmd:`status-get` command is sent to the
Control Agent or DDNS daemon.

The ``thread-pool-size``, ``packet-queue-size`` and
``packet-queue-statistics`` parameters are returned only when the
command is sent to DHCP servers with multi-threading enabled. These
three parameters and ``multi-threading-enabled`` are never returned when
the :isccmd:`status-get` command is sent to the Control Agent or DDNS daemon.

To learn more about the HA status information returned by the
:isccmd:`status-get` command, please refer to the :ref:`command-ha-status-get`
section.


.. isccmd:: server-tag-get
.. _command-server-tag-get:

The ``server-tag-get`` Command:
-------------------------------

The :isccmd:`server-tag-get` command returns the configured server tag of
the DHCPv4 or DHCPv6 server (:ref:`cb-sharing` explains the server tag concept).

.. isccmd:: config-backend-pull
.. _command-config-backend-pull:

The ``config-backend-pull`` Command:
------------------------------------

The :isccmd:`config-backend-pull` command triggers the polling of configuration backends
(which must be configured for this command to have an effect),
explained in :ref:`dhcp4-cb-json`.

.. isccmd:: version-get
.. _command-version-get:

The ``version-get`` Command
---------------------------

The :isccmd:`version-get` command returns extended information about the Kea
version; it is the same information available via the ``-V``
command-line argument. This command does not take any parameters.

::

   {
       "command": "version-get"
   }

Commands Supported by the DHCPv4 Server
=======================================

.. isccmd:: subnet4-select-test
.. _command-subnet4-select-test:

The ``subnet4-select-test`` Command
-----------------------------------

The :isccmd:`subnet4-select-test` provides a way to test DHCPv4 subnet selection based
on a set of input parameters typically supplied in a client packet.
Recognized parameters take strings and are:

 -  ``interface`` - the incoming interface name
 -  ``address`` - the client address
 -  ``relay`` - the relay/gateway address
 -  ``local`` - the local/destination address
 -  ``remote`` - the remote/source address
 -  ``link`` - the RAI link-selection address
 -  ``subnet`` - the subnet-selection address
 -  ``classes`` - (list of strings) client classes (allowing to select a guarded subnet)

The RAI link-selection is ignored when the ``ignore-rai-link-selection``
compatibility flag is ``true``. When it is not ignored it has precedence
over the subnet-selection.

Outside of errors possible results are:

 -  (empty) "no selected subnet"
 -  "selected shared network '<name>' starting with subnet '<subnet>' id <id>"
 -  "selected subnet '<subnet>' id <id>"

.. isccmd:: subnet4o6-select-test
.. _command-subnet4o6-select-test:

The ``subnet4o6-select-test`` Command
-------------------------------------

The :isccmd:`subnet4o6-select-test` provides a way to test DHCPv4-over-DHCPv6 subnet
selection based on a set of input parameters typically supplied in a client
packet. Recognized parameters take strings and are:

 -  ``interface`` - the incoming interface name of the DHCPv6 server
 -  ``interface-id`` - the binary content of the interface-id relay option
 -  ``address`` - the client address
 -  ``relay`` - the relay/gateway address
 -  ``local`` - the local/destination address
 -  ``remote`` - the remote/source IPv6 address of the DHCPv6 server
 -  ``link`` - the first relay link IPv6 address
 -  ``subnet`` - the subnet-selection address
 -  ``classes`` - (list of strings) client classes (allowing to select a guarded subnet)

According to the code only ``remote``, ``interface-id`` and ``interface``
selectors are used. In DHCPv4-over-DHCPv6 implementation ``interface`` and
``remote`` values are transmitted from the DHCPv6 server, ``interface-id``
and ``link`` are carried in the relay info part of the DHCPv6 packet so
are the same as for the DHCPv6 server.

Outside of errors possible results are:

 -  (empty) "no selected subnet"
 -  "selected shared network '<name>' starting with subnet '<subnet>' id <id>"
 -  "selected subnet '<subnet>' id <id>"

Commands Supported by the DHCPv6 Server
=======================================

.. isccmd:: subnet6-select-test
.. _command-subnet6-select-test:

The ``subnet6-select-test`` Command
-----------------------------------

The :isccmd:`subnet6-select-test` provides a way to test DHCPv6 subnet selection based
on a set of input parameters typically supplied in a client packet.
Recognized parameters take strings and are:

 -  ``interface`` - the incoming interface name
 -  ``interface-id`` - the binary content of the interface-id relay option
 -  ``remote`` - the remote/source address
 -  ``link`` - the first relay link address
 -  ``classes`` - (list of strings) client classes (allowing to select a guarded subnet)

Outside of errors possible results are:

 -  (empty) "no selected subnet"
 -  "selected shared network '<name>' starting with subnet '<subnet>' id <id>"
 -  "selected subnet '<subnet>' id <id>"

Commands Supported by the D2 Server
===================================

The D2 server supports only a subset of the DHCPv4/DHCPv6 server commands:

-  :isccmd:`build-report`

-  :isccmd:`config-get`

-  :isccmd:`config-hash-get`

-  :isccmd:`config-reload`

-  :isccmd:`config-set`

-  :isccmd:`config-test`

-  :isccmd:`config-write`

-  :isccmd:`list-commands`

-  :isccmd:`shutdown`

-  :isccmd:`status-get`

-  :isccmd:`version-get`

.. _agent-commands:

Commands Supported by the Control Agent
=======================================

The following commands, listed in :ref:`commands-common`, are also supported by the
Control Agent; when the ``service`` parameter is blank, the
commands are handled by the CA and they relate to the CA process itself:

-  :isccmd:`build-report`

-  :isccmd:`config-get`

-  :isccmd:`config-hash-get`

-  :isccmd:`config-reload`

-  :isccmd:`config-set`

-  :isccmd:`config-test`

-  :isccmd:`config-write`

-  :isccmd:`list-commands`

-  :isccmd:`shutdown`

-  :isccmd:`status-get`

-  :isccmd:`version-get`

.. _ctrl-channel-migration:

Migration from the Control Agent
================================

Since Kea version 2.7.2 DHCP servers support HTTP/HTTPS control channels
so the Control Agent (CA) is no longer needed.

The DHCPv4, DHCPv6, and D2 servers extend the ``control-socket`` entry
to ``control-sockets`` list. To migrate a CA configuration add an element
to this list with:

-  ``socket-type`` set to ``http`` or ``https``

-  ``socket-address`` with the content of CA ``http-host``

-  ``socket-port`` with the content of CA ``http-port``

-  ``trust-anchor`` (unchanged)

-  ``cert-file`` (unchanged)

-  ``key-file`` (unchanged)

-  ``cert-required`` (unchanged)

-  ``authentication`` (unchanged)

User context is supported too. Please look at respective HTTP control socket
sections for defaults and other details (beware that two servers must use
different address / port pairs): :ref:`dhcp4-http-ctrl-channel`,
:ref:`dhcp6-http-ctrl-channel` and :ref:`d2-http-ctrl-channel`

For compatibility the JSON result of these HTTP/HTTPS control sockets is
still encapsulated into a list.
