AT_BANNER([PMD])

m4_divert_push([PREPARE_TESTS])

# Given the output of `ovs-appctl dpif-netdev/pmd-rxq-show`, prints a list
# of every rxq (one per line) in the form:
# port_name rxq_id numa_id core_id
parse_pmd_rxq_show () {
    awk '/pmd thread/ {numa=$4; core=substr($6, 1, length($6) - 1)} /^  port:/ {print  $2, $4, numa, core}' | sort
}

# Given the output of `ovs-appctl dpif-netdev/pmd-rxq-show`,
# and with queues for each core on one line, prints the rxqs
# of the core on one line
# 'port:' port_name 'queue_id:' rxq_id rxq_id rxq_id rxq_id
parse_pmd_rxq_show_group () {
   awk '/port:/ {print  $1, $2, $3, $4, $13, $22, $31}'
}

# Given the output of `ovs-appctl dpctl/dump-flows`, prints a list of flows
# (one per line), with the pmd_id at the beginning of the line
#
flow_dump_prepend_pmd () {
    awk '/flow-dump from the main/ {pmd_id=-1; next} /flow-dump from pmd/ {pmd_id=$7; next} {print pmd_id, $0}' | sort
}

m4_divert_pop([PREPARE_TESTS])

dnl CHECK_CPU_DISCOVERED([n_cpu])
dnl
dnl Waits until CPUs discovered and checks if number of discovered CPUs
dnl is greater or equal to 'n_cpu'. Without parameters checks that at
dnl least one CPU discovered.
m4_define([CHECK_CPU_DISCOVERED], [
    PATTERN="Discovered [[0-9]]* NUMA nodes and [[0-9]]* CPU cores"
    OVS_WAIT_UNTIL([grep "$PATTERN" ovs-vswitchd.log])
    N_CPU=$(grep "$PATTERN" ovs-vswitchd.log | sed -e 's/.* \([[0-9]]*\) CPU cores/\1/')
    if [[ -z "$1" ]]
        then AT_CHECK([test "$N_CPU" -gt "0"])
        else AT_SKIP_IF([test "$N_CPU" -lt "$1"])
    fi
])

dnl CHECK_PMD_THREADS_CREATED([n_threads], [numa_id], [+line])
dnl
dnl Whaits for creation of 'n_threads' or at least 1 thread if $1 not
dnl passed. Checking starts from line number 'line' in ovs-vswithd.log .
m4_define([CHECK_PMD_THREADS_CREATED], [
    PATTERN="There are [[0-9]]* pmd threads on numa node $2"
    line_st=$3
    if [[ -z "$line_st" ]]
    then
        line_st="+0"
    fi
    OVS_WAIT_UNTIL([tail -n $line_st ovs-vswitchd.log | grep "$PATTERN"])
    N_THREADS=$(tail -n $line_st ovs-vswitchd.log | grep "$PATTERN" | tail -1 | sed -e 's/.* \([[0-9]]*\) pmd .*/\1/')
    if [[ -z "$1" ]]
        then AT_CHECK([test "$N_THREADS" -gt 0])
        else AT_CHECK([test "$N_THREADS" -eq "$1"])
    fi
])

dnl CHECK_DP_SLEEP_MAX([max_sleep], [enabled], [+line])
dnl
dnl Checks correct pmd load based sleep is set for the datapath.
dnl Checking starts from line number 'line' in ovs-vswithd.log .
m4_define([CHECK_DP_SLEEP_MAX], [
    SLEEP_TIME="PMD max sleep request is $1 usecs."
    SLEEP_STATE="PMD load based sleeps are $2."
    line_st=$3
    if [[ -z "$line_st" ]]
    then
        line_st="+0"
    fi
    OVS_WAIT_UNTIL([tail -n $line_st ovs-vswitchd.log | grep "$SLEEP_TIME"])
    OVS_WAIT_UNTIL([tail -n $line_st ovs-vswitchd.log | grep "$SLEEP_STATE"])
])

m4_define([SED_NUMA_CORE_PATTERN], ["s/\(numa_id \)[[0-9]]*\( core_id \)[[0-9]]*:/\1<cleared>\2<cleared>:/"])
m4_define([DUMMY_NUMA], [--dummy-numa="0,0,0,0"])

AT_SETUP([PMD - creating a thread/add-port])
OVS_VSWITCHD_START([add-port br0 p0 -- set Interface p0 type=dummy-pmd], [], [], [DUMMY_NUMA])

CHECK_CPU_DISCOVERED()
CHECK_PMD_THREADS_CREATED()

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | sed SED_NUMA_CORE_PATTERN], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id <cleared> core_id <cleared>:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
])

AT_CHECK([ovs-appctl dpif/show | sed 's/\(tx_queues=\)[[0-9]]*/\1<cleared>/g'], [0], [dnl
dummy@ovs-dummy: hit:0 missed:0
  br0:
    br0 65534/100: (dummy-internal)
    p0 1/1: (dummy-pmd: configured_rx_queues=1, configured_tx_queues=<cleared>, requested_rx_queues=1, requested_tx_queues=<cleared>)
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - multiqueue support])
OVS_VSWITCHD_START([add-port br0 p0 -- set Interface p0 type=dummy-pmd], [], [], [DUMMY_NUMA])

CHECK_CPU_DISCOVERED()
CHECK_PMD_THREADS_CREATED()

AT_CHECK([ovs-vsctl set interface p0 options:n_rxq=8])

AT_CHECK([ovs-appctl dpif/show | sed 's/\(tx_queues=\)[[0-9]]*/\1<cleared>/g'], [0], [dnl
dummy@ovs-dummy: hit:0 missed:0
  br0:
    br0 65534/100: (dummy-internal)
    p0 1/1: (dummy-pmd: configured_rx_queues=8, configured_tx_queues=<cleared>, requested_rx_queues=8, requested_tx_queues=<cleared>)
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | sed SED_NUMA_CORE_PATTERN], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id <cleared> core_id <cleared>:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  1 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  2 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  3 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  4 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  5 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  6 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  7 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
])

OVS_VSWITCHD_STOP
AT_CLEANUP


AT_SETUP([PMD - pmd-cpu-mask/distribution of rx queues])
OVS_VSWITCHD_START([add-port br0 p0 -- set Interface p0 type=dummy-pmd options:n_rxq=8],
                   [], [], [DUMMY_NUMA])

CHECK_CPU_DISCOVERED(2)
CHECK_PMD_THREADS_CREATED()

AT_CHECK([ovs-appctl dpif/show | sed 's/\(tx_queues=\)[[0-9]]*/\1<cleared>/g'], [0], [dnl
dummy@ovs-dummy: hit:0 missed:0
  br0:
    br0 65534/100: (dummy-internal)
    p0 1/1: (dummy-pmd: configured_rx_queues=8, configured_tx_queues=<cleared>, requested_rx_queues=8, requested_tx_queues=<cleared>)
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | sed SED_NUMA_CORE_PATTERN], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id <cleared> core_id <cleared>:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  1 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  2 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  3 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  4 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  5 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  6 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  7 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=roundrobin])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using roundrobin algorithm"])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0x3])
CHECK_PMD_THREADS_CREATED([2], [], [+$TMP])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | sort], [0], [dnl
port: p0 queue-id: 0 2 4 6
port: p0 queue-id: 1 3 5 7
])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=cycles])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using cycles algorithm"])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | sort], [0], [dnl
port: p0 queue-id: 0 3 4 7
port: p0 queue-id: 1 2 5 6
])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=group])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using group algorithm"])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | sort], [0], [dnl
port: p0 queue-id: 0 2 4 6
port: p0 queue-id: 1 3 5 7
])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0x1])
CHECK_PMD_THREADS_CREATED([1], [], [+$TMP])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | sed SED_NUMA_CORE_PATTERN], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id <cleared> core_id <cleared>:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  1 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  2 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  3 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  4 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  5 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  6 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  7 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - pmd-cpu-mask - dual NUMA])
OVS_VSWITCHD_START([add-port br0 p0 -- set Interface p0 type=dummy-pmd options:n_rxq=8 options:numa_id=1 -- set Open_vSwitch . other_config:pmd-cpu-mask=1],
                   [], [], [--dummy-numa 1,1,0,0])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
CHECK_CPU_DISCOVERED(4)
CHECK_PMD_THREADS_CREATED()

AT_CHECK([ovs-appctl dpif/show | sed 's/\(tx_queues=\)[[0-9]]*/\1<cleared>/g'], [0], [dnl
dummy@ovs-dummy: hit:0 missed:0
  br0:
    br0 65534/100: (dummy-internal)
    p0 1/1: (dummy-pmd: configured_rx_queues=8, configured_tx_queues=<cleared>, requested_rx_queues=8, requested_tx_queues=<cleared>)
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | sed SED_NUMA_CORE_PATTERN], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id <cleared> core_id <cleared>:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  1 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  2 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  3 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  4 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  5 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  6 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  7 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
])

# Force cross-numa polling
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0xc])
CHECK_PMD_THREADS_CREATED([2], [0], [+$TMP])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using cycles algorithm"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "There's no available (non-isolated) pmd thread on numa node 1. Port 'p0' rx queue 7 will be assigned to a pmd on numa node 0. This may lead to reduced performance."])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | sort], [0], [dnl
port: p0 queue-id: 0 3 4 7
port: p0 queue-id: 1 2 5 6
])

# Check other assignment types for cross-numa polling
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=roundrobin])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using roundrobin algorithm"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "There's no available (non-isolated) pmd thread on numa node 1. Port 'p0' rx queue 7 will be assigned to a pmd on numa node 0. This may lead to reduced performance."])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | sort], [0], [dnl
port: p0 queue-id: 0 2 4 6
port: p0 queue-id: 1 3 5 7
])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=group])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using group algorithm"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "There's no available (non-isolated) pmd thread on numa node 1. Port 'p0' rx queue 7 will be assigned to a pmd on numa node 0. This may lead to reduced performance."])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | sort], [0], [dnl
port: p0 queue-id: 0 2 4 6
port: p0 queue-id: 1 3 5 7
])

# Switch back to same numa
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0x3])
CHECK_PMD_THREADS_CREATED([2], [1], [+$TMP])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using group algorithm"])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | sort], [0], [dnl
port: p0 queue-id: 0 2 4 6
port: p0 queue-id: 1 3 5 7
])

# Check local numa is only used if available
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0x6])
CHECK_PMD_THREADS_CREATED([1], [0], [+$TMP])
CHECK_PMD_THREADS_CREATED([1], [1], [+$TMP])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using group algorithm"])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id 1 core_id 1:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  1 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  2 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  3 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  4 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  5 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  6 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  7 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
pmd thread numa_id 0 core_id 2:
  isolated : false
])


# Check other assignment types
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=roundrobin])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using roundrobin algorithm"])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id 1 core_id 1:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  1 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  2 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  3 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  4 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  5 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  6 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  7 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
pmd thread numa_id 0 core_id 2:
  isolated : false
])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=cycles])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using cycles algorithm"])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id 1 core_id 1:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  1 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  2 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  3 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  4 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  5 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  6 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  7 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
pmd thread numa_id 0 core_id 2:
  isolated : false
])

# Switch back from mixed numa to single numa
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0x1])
CHECK_PMD_THREADS_CREATED([1], [1], [+$TMP])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show], [0], [dnl
Displaying last 60 seconds pmd usage %
pmd thread numa_id 1 core_id 0:
  isolated : false
  port: p0                queue-id:  0 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  1 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  2 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  3 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  4 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  5 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  6 (enabled)   pmd usage: NOT AVAIL
  port: p0                queue-id:  7 (enabled)   pmd usage: NOT AVAIL
  overhead: NOT AVAIL
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - pmd-cpu-mask - multi NUMA])
OVS_VSWITCHD_START([add-port br0 p0 \
                    -- set Interface p0 type=dummy-pmd options:n_rxq=4 \
                    -- set Interface p0 options:numa_id=0 \
                    -- set Open_vSwitch . other_config:pmd-cpu-mask=0xf \
                    -- set open_vswitch . other_config:pmd-rxq-assign=cycles],
                   [], [], [--dummy-numa 1,2,1,2])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=group])

OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using group algorithm"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "There's no available (non-isolated) pmd thread on numa node 0."])

# check all pmds from both non-local numas are assigned an rxq
AT_CHECK([test `ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | wc -l` -eq 4])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=cycles])

OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using cycles algorithm"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "There's no available (non-isolated) pmd thread on numa node 0."])

# check all pmds from both non-local numas are assigned an rxq
AT_CHECK([test `ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | wc -l` -eq 4])

TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=roundrobin])

OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using roundrobin algorithm"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "There's no available (non-isolated) pmd thread on numa node 0."])

# check all pmds from both non-local numas are assigned an rxq
AT_CHECK([test `ovs-appctl dpif-netdev/pmd-rxq-show | awk '/AVAIL$/ { printf("%s\t", $0); next } 1' | parse_pmd_rxq_show_group | wc -l` -eq 4])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - stats])
OVS_VSWITCHD_START([add-port br0 p0 -- set Interface p0 ofport_request=7 type=dummy-pmd options:n_rxq=4],
                   [], [], [DUMMY_NUMA])

CHECK_CPU_DISCOVERED()
CHECK_PMD_THREADS_CREATED()

AT_CHECK([ovs-appctl vlog/set dpif_netdev:dbg])
AT_CHECK([ovs-ofctl add-flow br0 action=normal])
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:emc-insert-inv-prob=1])
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:smc-enable=true])

sleep 1

AT_CHECK([ovs-appctl dpif/show | sed 's/\(tx_queues=\)[[0-9]]*/\1<cleared>/g'], [0], [dnl
dummy@ovs-dummy: hit:0 missed:0
  br0:
    br0 65534/100: (dummy-internal)
    p0 7/1: (dummy-pmd: configured_rx_queues=4, configured_tx_queues=<cleared>, requested_rx_queues=4, requested_tx_queues=<cleared>)
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-stats-show | sed SED_NUMA_CORE_PATTERN | sed '/cycles/d' | grep pmd -A 12], [0], [dnl
pmd thread numa_id <cleared> core_id <cleared>:
  packets received: 0
  packet recirculations: 0
  avg. datapath passes per packet: 0.00
  phwol hits: 0
  mfex opt hits: 0
  simple match hits: 0
  emc hits: 0
  smc hits: 0
  megaflow hits: 0
  avg. subtable lookups per megaflow hit: 0.00
  miss with success upcall: 0
  miss with failed upcall: 0
])

ovs-appctl time/stop
ovs-appctl time/warp 100
(
for i in `seq 0 19`;
    do
    pkt="in_port(7),eth(src=50:54:00:00:00:77,dst=50:54:00:00:01:78),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)"
    AT_CHECK([ovs-appctl netdev-dummy/receive p0 $pkt])
    done
)
ovs-appctl time/warp 100

AT_CHECK([grep -A 1 'miss upcall' ovs-vswitchd.log | tail -n 1], [0], [dnl
recirc_id(0),dp_hash(0),skb_priority(0),in_port(1),skb_mark(0),ct_state(0),ct_zone(0),ct_mark(0),ct_label(0),packet_type(ns=0,id=0),eth(src=50:54:00:00:00:77,dst=50:54:00:00:01:78),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)
])
AT_CHECK([cat ovs-vswitchd.log | filter_flow_install | strip_xout], [0], [dnl
recirc_id(0),in_port(1),packet_type(ns=0,id=0),eth(src=50:54:00:00:00:77,dst=50:54:00:00:01:78),eth_type(0x0800),ipv4(frag=no), actions: <del>
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-stats-show | sed SED_NUMA_CORE_PATTERN | sed '/cycles/d' | grep pmd -A 12], [0], [dnl
pmd thread numa_id <cleared> core_id <cleared>:
  packets received: 20
  packet recirculations: 0
  avg. datapath passes per packet: 1.00
  phwol hits: 0
  mfex opt hits: 0
  simple match hits: 0
  emc hits: 19
  smc hits: 0
  megaflow hits: 0
  avg. subtable lookups per megaflow hit: 0.00
  miss with success upcall: 1
  miss with failed upcall: 0
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - pmd-rxq-show pmd usage time])
OVS_VSWITCHD_START([add-port br0 p0 -- set Interface p0 type=dummy-pmd], [], [], [DUMMY_NUMA])

#CHECK_CPU_DISCOVERED()
#CHECK_PMD_THREADS_CREATED()

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | grep Displaying], [0], [dnl
Displaying last 60 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs -1 | grep Displaying], [0], [dnl
Displaying last 60 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 0 | grep Displaying], [0], [dnl
Displaying last 60 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 1 | grep Displaying], [0], [dnl
Displaying last 5 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 5 | grep Displaying], [0], [dnl
Displaying last 5 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 6 | grep Displaying], [0], [dnl
Displaying last 10 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 51 | grep Displaying], [0], [dnl
Displaying last 55 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 55 | grep Displaying], [0], [dnl
Displaying last 55 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 56 | grep Displaying], [0], [dnl
Displaying last 60 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 60 | grep Displaying], [0], [dnl
Displaying last 60 seconds pmd usage %
])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show -secs 61 | grep Displaying], [0], [dnl
Displaying last 60 seconds pmd usage %
])

OVS_VSWITCHD_STOP
AT_CLEANUP

dnl Reconfigure the number of rx queues of a port, make sure that all the
dnl queues are polled by the datapath and try to send a couple of packets.
AT_SETUP([PMD - reconfigure n_rxq])
OVS_VSWITCHD_START(
  [add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=2 -- \
   add-port br0 p2 -- set Interface p2 type=dummy-pmd ofport_request=2
], [], [], [--dummy-numa 0])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-ofctl add-flow br0 action=controller])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
p1 1 0 0
p2 0 0 0
])

AT_CAPTURE_FILE([ofctl_monitor.log])
AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 1 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

AT_CHECK([ovs-vsctl set interface p1 options:n_rxq=4])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
p1 1 0 0
p1 2 0 0
p1 3 0 0
p2 0 0 0
])

AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 3 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

dnl Check resetting to default number of rx queues after removal from the db.
AT_CHECK([ovs-vsctl remove interface p1 options n_rxq])

AT_CHECK([ovs-appctl dpif/show | grep p1 | sed 's/\(tx_queues=\)[[0-9]]*/\1<cleared>/g'], [0], [dnl
    p1 1/1: (dummy-pmd: configured_rx_queues=1, configured_tx_queues=<cleared>, requested_rx_queues=1, requested_tx_queues=<cleared>)
])

OVS_VSWITCHD_STOP
AT_CLEANUP

dnl There was a bug where OVS failed to create a ukey and install a megaflow
dnl if a packet with the exact same flow was received by two different pmd
dnl threads.  This is a regression test for that bug.
AT_SETUP([PMD - same flow multiple threads])
OVS_VSWITCHD_START(
  [add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=2 -- \
   set Open_vSwitch . other_config:pmd-cpu-mask=3
], [], [], [--dummy-numa 0,0])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-ofctl add-flow br0 action=controller])

dnl Make sure that the queues are on different cores.  There's no way to
dnl control which queue is on which thread, we just need to make sure that
dnl two threads (core_id) show up in pmd-rxq-show
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show | cut -f 4 -d ' ' | sort], [0], [dnl
0
1
])

AT_CAPTURE_FILE([ofctl_monitor.log])
AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 1 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 4])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

dnl Make sure that both flows have been installed
AT_CHECK([ovs-appctl dpctl/dump-flows | flow_dump_prepend_pmd], [0], [dnl
0 recirc_id(0),in_port(1),packet_type(ns=0,id=0),eth_type(0x0800),ipv4(frag=no), packets:0, bytes:0, used:never, actions:userspace(pid=0,controller(reason=1,dont_send=0,continuation=0,recirc_id=1,rule_cookie=0,controller_id=0,max_len=65535))
1 recirc_id(0),in_port(1),packet_type(ns=0,id=0),eth_type(0x0800),ipv4(frag=no), packets:0, bytes:0, used:never, actions:userspace(pid=0,controller(reason=1,dont_send=0,continuation=0,recirc_id=1,rule_cookie=0,controller_id=0,max_len=65535))
])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - change numa node])
OVS_VSWITCHD_START(
  [add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=2 -- \
   add-port br0 p2 -- set Interface p2 type=dummy-pmd ofport_request=2 options:n_rxq=2 -- \
   set Open_vSwitch . other_config:pmd-cpu-mask=7
], [], [], [--dummy-numa 0,1,8])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-ofctl add-flow br0 action=controller])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
p1 1 0 0
p2 0 0 0
p2 1 0 0
])

AT_CAPTURE_FILE([ofctl_monitor.log])
AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p2 --qid 1 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=2 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

AT_CHECK([ovs-vsctl set Interface p2 options:numa_id=1])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
p1 1 0 0
p2 0 1 1
p2 1 1 1
])

AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 1 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p2 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=2 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

AT_CHECK([ovs-vsctl set Interface p1 options:numa_id=8])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 8 2
p1 1 8 2
p2 0 1 1
p2 1 1 1
])

AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 1 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p2 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=2 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])


OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - non pmd device])
OVS_VSWITCHD_START(
  [add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=1 -- \
   add-port br0 p2 -- set Interface p2 type=dummy ofport_request=2 -- \
   set Interface br0 options:tx_pcap=br0.pcap -- \
   set Open_vSwitch . other_config:pmd-cpu-mask=1
], [], [], [--dummy-numa 0,0])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-ofctl add-flow br0 actions=LOCAL])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

AT_CHECK([ovs-appctl netdev-dummy/receive p2 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `ovs-pcap br0.pcap | wc -l` -ge 2])

AT_CHECK([ovs-pcap br0.pcap], [0], [dnl
50540000000a50540000000908004500005c000000004001669f0a0000020a000001080013fc00000000000102030405060708090a0b0c0d0e0f101112131415161718191a1b1c1d1e1f202122232425262728292a2b2c2d2e2f303132333435363738393a3b3c3d3e3f
50540000000a50540000000908004500005c000000004001669f0a0000020a000001080013fc00000000000102030405060708090a0b0c0d0e0f101112131415161718191a1b1c1d1e1f202122232425262728292a2b2c2d2e2f303132333435363738393a3b3c3d3e3f
])

AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=2])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 1
])

AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

AT_CHECK([ovs-appctl netdev-dummy/receive p2 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `ovs-pcap br0.pcap | wc -l` -ge 4])

AT_CHECK([ovs-pcap br0.pcap], [0], [dnl
50540000000a50540000000908004500005c000000004001669f0a0000020a000001080013fc00000000000102030405060708090a0b0c0d0e0f101112131415161718191a1b1c1d1e1f202122232425262728292a2b2c2d2e2f303132333435363738393a3b3c3d3e3f
50540000000a50540000000908004500005c000000004001669f0a0000020a000001080013fc00000000000102030405060708090a0b0c0d0e0f101112131415161718191a1b1c1d1e1f202122232425262728292a2b2c2d2e2f303132333435363738393a3b3c3d3e3f
50540000000a50540000000908004500005c000000004001669f0a0000020a000001080013fc00000000000102030405060708090a0b0c0d0e0f101112131415161718191a1b1c1d1e1f202122232425262728292a2b2c2d2e2f303132333435363738393a3b3c3d3e3f
50540000000a50540000000908004500005c000000004001669f0a0000020a000001080013fc00000000000102030405060708090a0b0c0d0e0f101112131415161718191a1b1c1d1e1f202122232425262728292a2b2c2d2e2f303132333435363738393a3b3c3d3e3f
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - add remove ports])
OVS_VSWITCHD_START(
  [], [], [], [--dummy-numa 0,0])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-ofctl add-flow br0 actions=controller])

AT_CHECK([ovs-vsctl add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=1])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
])

AT_CAPTURE_FILE([ofctl_monitor.log])
AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

AT_CHECK([ovs-vsctl del-port br0 p1])
AT_CHECK([ovs-vsctl add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=1])

AT_CHECK([ovs-ofctl monitor br0 65534 invalid_ttl --detach --no-chdir --pidfile 2> ofctl_monitor.log])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 --qid 0 'in_port(1),eth(src=50:54:00:00:00:09,dst=50:54:00:00:00:0a),eth_type(0x0800),ipv4(src=10.0.0.2,dst=10.0.0.1,proto=1,tos=0,ttl=64,frag=no),icmp(type=8,code=0)'])

OVS_WAIT_UNTIL([test `wc -l < ofctl_monitor.log` -ge 2])
OVS_WAIT_UNTIL([ovs-appctl -t ovs-ofctl exit])

AT_CHECK([cat ofctl_monitor.log], [0], [dnl
NXT_PACKET_IN2 (xid=0x0): cookie=0x0 total_len=106 in_port=1 (via action) data_len=106 (unbuffered)
icmp,vlan_tci=0x0000,dl_src=50:54:00:00:00:09,dl_dst=50:54:00:00:00:0a,nw_src=10.0.0.2,nw_dst=10.0.0.1,nw_tos=0,nw_ecn=0,nw_ttl=64,nw_frag=no,icmp_type=8,icmp_code=0 icmp_csum:13fc
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - rxq affinity])
OVS_VSWITCHD_START(
  [], [], [], [--dummy-numa 0,0,0,0,0,0,0,0,0])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-ofctl add-flow br0 actions=controller])

AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0x1fe])

AT_CHECK([ovs-vsctl add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=4 other_config:pmd-rxq-affinity="0:3,1:7,2:2,3:8"])

dnl The rxqs should be on the requested cores.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 3
p1 1 0 7
p1 2 0 2
p1 3 0 8
])

AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=6])

dnl We removed the cores requested by some queues from pmd-cpu-mask.
dnl Those queues will be polled by remaining non-isolated pmds.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 1
p1 1 0 1
p1 2 0 2
p1 3 0 1
])

# Check they are pinned when those pmds are available again
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0x1fe])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 3
p1 1 0 7
p1 2 0 2
p1 3 0 8
])

AT_CHECK([ovs-vsctl remove Interface p1 other_config pmd-rxq-affinity])

dnl We removed the rxq-affinity request.  dpif-netdev should assign queues
dnl in a round robin fashion.  We just make sure that every rxq is being
dnl polled again.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show | cut -f 1,2 -d ' ' | sort], [0], [dnl
p1 0
p1 1
p1 2
p1 3
])

AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=6])
AT_CHECK([ovs-vsctl set Interface p1 other_config:pmd-rxq-affinity='0:1'])

dnl We explicitly requested core 1 for queue 0.  Core 1 becomes isolated and
dnl every other queue goes to core 2.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 1
p1 1 0 2
p1 2 0 2
p1 3 0 2
])

OVS_VSWITCHD_STOP(["/cannot be pinned with port/d"])
AT_CLEANUP

AT_SETUP([PMD - rxq affinity - non-isolate])
OVS_VSWITCHD_START(
  [], [], [], [--dummy-numa 0,0,0,0,0,0,0,0,0])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-ofctl add-flow br0 actions=controller])

AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=0x1fe])

AT_CHECK([ovs-vsctl add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=4 other_config:pmd-rxq-affinity="0:3,1:7,2:2,3:8"])

dnl The rxqs should be on the requested cores.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 3
p1 1 0 7
p1 2 0 2
p1 3 0 8
])

# change rxq assignment algorithm
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=group])

dnl The rxqs should be on the requested cores.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 3
p1 1 0 7
p1 2 0 2
p1 3 0 8
])

# try to pin & non-isolate
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-isolate=false])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "pmd-rxq-affinity does not isolate PMD core"])

# should not impact - all rxqs are still pinned
dnl The rxqs should be on the requested cores.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 3
p1 1 0 7
p1 2 0 2
p1 3 0 8
])

# remove some pinning - see if non-isolate pmd are used for ovs rxq assignment of other rxqs
AT_CHECK([ovs-vsctl remove Interface p1 other_config pmd-rxq-affinity])
AT_CHECK([ovs-vsctl set Interface p1 other_config:pmd-rxq-affinity='0:1'])
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=6])

dnl We explicitly requested core 1 for queue 0.  Core 1 is not isolated so it is
dnl use for other rxqs.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 1
p1 1 0 2
p1 2 0 1
p1 3 0 2
])

# change to algorithm that does not support pin & non-isolate
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=cycles])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "pmd-rxq-isolate can only be set false when using pmd-rxq-assign=group"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "pmd-rxq-affinity isolates PMD core"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using cycles algorithm"])

dnl We explicitly requested core 1 for queue 0.  Core 1 becomes isolated and
dnl every other queue goes to core 2.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 1
p1 1 0 2
p1 2 0 2
p1 3 0 2
])

# change rxq assignment algorithm to one that support pin & non-isolate
TMP=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-rxq-assign=group])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "pmd-rxq-affinity does not isolate PMD core"])
OVS_WAIT_UNTIL([tail -n +$TMP ovs-vswitchd.log | grep "Performing pmd to rx queue assignment using group algorithm"])

#dnl We explicitly requested core 1 for queue 0.  Core 1 becomes isolated and
#dnl every other queue goes to core 2.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 1
p1 1 0 2
p1 2 0 1
p1 3 0 2
])

OVS_VSWITCHD_STOP(["/cannot be pinned with port/d
/pmd-rxq-isolate can only be set false when using pmd-rxq-assign=group/d"])
AT_CLEANUP


AT_SETUP([PMD - rxq affinity - NUMA])
OVS_VSWITCHD_START(
  [], [], [], [--dummy-numa 0,0,0,1,1,8,8])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-ofctl add-flow br0 actions=controller])

AT_CHECK([ovs-vsctl set Open_vSwitch . other_config:pmd-cpu-mask=7e])

AT_CHECK([ovs-vsctl add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=2 options:numa_id=0 other_config:pmd-rxq-affinity="0:1,1:2"])

dnl The rxqs should be on the requested cores.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 1
p1 1 0 2
])

AT_CHECK([ovs-vsctl set Interface p1 other_config:pmd-rxq-affinity="0:3,1:4"])

dnl We moved the queues to different contiguous numa node. Expecting threads on
dnl NUMA node 1 to be created.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 1 3
p1 1 1 4
])

AT_CHECK([ovs-vsctl set Interface p1 other_config:pmd-rxq-affinity="0:5,1:6"])

dnl We moved the queues to different non-contiguous numa node. Expecting threads on
dnl NUMA node 8 to be created.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 8 5
p1 1 8 6
])

AT_CHECK([ovs-vsctl set Interface p1 other_config:pmd-rxq-affinity="0:3,1:1"])

dnl Queues splitted between contiguous NUMA nodes.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 1 3
p1 1 0 1
])

AT_CHECK([ovs-vsctl set Interface p1 other_config:pmd-rxq-affinity="0:5,1:1"])

dnl Queues splitted between non-contiguous NUMA nodes.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 8 5
p1 1 0 1
])

AT_CHECK([ovs-vsctl remove Interface p1 other_config pmd-rxq-affinity])

dnl We removed the rxq-affinity request.  dpif-netdev should assign queues
dnl in a round robin fashion.  We just make sure that every rxq is being
dnl polled again.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show | cut -f 1,2 -d ' ' | sort], [0], [dnl
p1 0
p1 1
])

AT_CHECK([ovs-vsctl set Interface p1 other_config:pmd-rxq-affinity='0:3'])

dnl We explicitly requesting NUMA node 1 for queue 0.
dnl Queue 1 should be polled by thread from NUMA node 0.
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show | cut -f 1,2,3 -d ' '], [0], [dnl
p1 0 1
p1 1 0
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - monitor threads])
OVS_VSWITCHD_START(
  [], [], [], [--dummy-numa 0,0])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

dnl The two devices are connected together externally using net.sock
AT_CHECK([ovs-vsctl add-port br0 p1 -- set Interface p1 type=dummy-pmd ofport_request=1 options:n_rxq=1 options:pstream=punix:$OVS_RUNDIR/net.sock])
AT_CHECK([ovs-vsctl add-port br0 p2 -- set Interface p2 type=dummy-pmd ofport_request=2 options:n_rxq=1 options:stream=unix:$OVS_RUNDIR/net.sock])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
p2 0 0 0
])

dnl Enable bfd with a very aggressive interval. This will make the monitor very
dnl busy, and uncover race conditions with the main thread.
AT_CHECK([ovs-vsctl set Interface p1 bfd:enable=true bfd:min_rx=1 bfd:min_tx=1])
AT_CHECK([ovs-vsctl set Interface p2 bfd:enable=true bfd:min_rx=1 bfd:min_tx=1])

AT_CHECK([ovs-vsctl wait-until Interface p1 bfd_status:forwarding=true \
                 -- wait-until Interface p2 bfd_status:forwarding=true])

dnl Trigger reconfiguration of the datapath
AT_CHECK([ovs-vsctl set Interface p1 options:n_rxq=2])
AT_CHECK([ovs-vsctl set Interface p2 options:n_rxq=2])

dnl Make sure that reconfiguration succeded
AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
p1 1 0 0
p2 0 0 0
p2 1 0 0
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - dpctl])
OVS_VSWITCHD_START(
  [del-br br0], [], [], [--dummy-numa 0,0])
AT_CHECK([ovs-appctl vlog/set dpif:dbg dpif_netdev:dbg])

AT_CHECK([ovs-appctl dpctl/add-dp dummy@dp0])
AT_CHECK([ovs-appctl dpctl/add-if dummy@dp0 p1,type=dummy-pmd])
AT_CHECK([ovs-appctl dpctl/add-if dummy@dp0 p2,type=dummy])

AT_CHECK([ovs-appctl dpif-netdev/pmd-rxq-show dp0 | parse_pmd_rxq_show], [0], [dnl
p1 0 0 0
])

AT_CHECK([ovs-appctl dpctl/show dummy@dp0], [0], [dnl
dummy@dp0:
  lookups: hit:0 missed:0 lost:0
  flows: 0
  port 0: dp0 (dummy-internal)
  port 1: p1 (dummy-pmd: configured_rx_queues=1, configured_tx_queues=1, requested_rx_queues=1, requested_tx_queues=1)
  port 2: p2 (dummy)
])

AT_CHECK([ovs-appctl dpctl/add-flow dummy@dp0 'in_port(1),eth(src=00:00:00:00:00:01,dst=00:00:00:00:00:02),eth_type(0x1234)' 2], [0], [dnl
])

AT_CHECK([ovs-appctl dpctl/dump-flows dummy@dp0 | sort], [0], [dnl
flow-dump from pmd on cpu core: 0
flow-dump from the main thread:
recirc_id(0),in_port(1),eth(src=00:00:00:00:00:01,dst=00:00:00:00:00:02),eth_type(0x1234), packets:0, bytes:0, used:never, actions:2
recirc_id(0),in_port(1),eth(src=00:00:00:00:00:01,dst=00:00:00:00:00:02),eth_type(0x1234), packets:0, bytes:0, used:never, actions:2
])

dnl Check pmd filtering option.
AT_CHECK([ovs-appctl dpctl/dump-flows dummy@dp0 pmd=0], [0], [dnl
recirc_id(0),in_port(1),eth(src=00:00:00:00:00:01,dst=00:00:00:00:00:02),eth_type(0x1234), packets:0, bytes:0, used:never, actions:2
])

AT_CHECK([ovs-appctl dpctl/dump-flows dummy@dp0 pmd=-1], [0], [dnl
recirc_id(0),in_port(1),eth(src=00:00:00:00:00:01,dst=00:00:00:00:00:02),eth_type(0x1234), packets:0, bytes:0, used:never, actions:2
])

AT_CHECK([ovs-appctl dpctl/del-flow dummy@dp0 'in_port(1),eth(src=00:00:00:00:00:01,dst=00:00:00:00:00:02),eth_type(0x1234)'], [0], [dnl
])

AT_CHECK([ovs-appctl dpctl/dump-flows dummy@dp0], [0], [dnl
])

AT_CHECK([ovs-appctl dpctl/del-dp dummy@dp0], [0], [dnl
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - dpif configuration])
OVS_VSWITCHD_START([], [], [], [--dummy-numa 0,0])
AT_CHECK([ovs-vsctl add-port br0 p1 -- set Interface p1 type=dummy-pmd])

AT_CHECK([ovs-appctl dpif-netdev/dpif-impl-set dpif_scalar], [0], [dnl
DPIF implementation set to dpif_scalar.
])

AT_CHECK([ovs-vsctl show], [], [stdout])
AT_CHECK([ovs-appctl dpif-netdev/dpif-impl-get | grep "dpif_scalar"], [], [dnl
  dpif_scalar (pmds: 0)
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - dpcls configuration])
OVS_VSWITCHD_START([], [], [], [--dummy-numa 0,0])
AT_CHECK([ovs-vsctl add-port br0 p1 -- set Interface p1 type=dummy-pmd])

AT_CHECK([ovs-vsctl show], [], [stdout])
AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-prio-set autovalidator 3], [0], [dnl
Lookup priority change affected 0 dpcls ports and 0 subtables.
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-info-get | grep autovalidator], [], [dnl
  autovalidator (Use count: 0, Priority: 3)
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-prio-set generic 4], [0], [dnl
Lookup priority change affected 0 dpcls ports and 0 subtables.
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-info-get | grep generic], [], [dnl
  generic (Use count: 0, Priority: 4)
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-prio-set generic 8], [0], [dnl
Lookup priority change affected 0 dpcls ports and 0 subtables.
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-info-get | grep generic], [], [dnl
  generic (Use count: 0, Priority: 8)
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-prio-set autovalidator 8], [0], [dnl
Lookup priority change affected 0 dpcls ports and 0 subtables.
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-info-get | grep autovalidator], [], [dnl
  autovalidator (Use count: 0, Priority: 8)
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-prio-set generic 0], [0], [dnl
Lookup priority change affected 0 dpcls ports and 0 subtables.
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-info-get | grep generic], [], [dnl
  generic (Use count: 0, Priority: 0)
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-prio-set generic 255], [0], [dnl
Lookup priority change affected 0 dpcls ports and 0 subtables.
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-info-get | grep generic], [], [dnl
  generic (Use count: 0, Priority: 255)
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-prio-set generic -1], [2],
[], [dnl
error converting priority, use integer in range 0-255
ovs-appctl: ovs-vswitchd: server returned an error
])

AT_CHECK([ovs-appctl dpif-netdev/subtable-lookup-prio-set generic 300], [2],
[], [dnl
error converting priority, use integer in range 0-255
ovs-appctl: ovs-vswitchd: server returned an error
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - pmd sleep])
OVS_VSWITCHD_START

dnl Check default
CHECK_DP_SLEEP_MAX([0], [disabled], [])

AT_CHECK([ovs-appctl dpif-netdev/pmd-sleep-show], [0], [dnl
Default max sleep:    0 us
])

dnl Check low value max sleep
get_log_next_line_num
AT_CHECK([ovs-vsctl set open_vswitch . other_config:pmd-sleep-max="1"])
CHECK_DP_SLEEP_MAX([1], [enabled], [+$LINENUM])
AT_CHECK([ovs-appctl dpif-netdev/pmd-sleep-show], [0], [dnl
Default max sleep:    1 us
])

dnl Check high value max sleep
get_log_next_line_num
AT_CHECK([ovs-vsctl set open_vswitch . other_config:pmd-sleep-max="10000"])
CHECK_DP_SLEEP_MAX([10000], [enabled], [+$LINENUM])
AT_CHECK([ovs-appctl dpif-netdev/pmd-sleep-show], [0], [dnl
Default max sleep: 10000 us
])

dnl Check setting max sleep to zero
get_log_next_line_num
AT_CHECK([ovs-vsctl set open_vswitch . other_config:pmd-sleep-max="0"])
CHECK_DP_SLEEP_MAX([0], [disabled], [+$LINENUM])
AT_CHECK([ovs-appctl dpif-netdev/pmd-sleep-show], [0], [dnl
Default max sleep:    0 us
])

dnl Check above high value max sleep
get_log_next_line_num
AT_CHECK([ovs-vsctl set open_vswitch . other_config:pmd-sleep-max="10001"])
CHECK_DP_SLEEP_MAX([10000], [enabled], [+$LINENUM])
AT_CHECK([ovs-appctl dpif-netdev/pmd-sleep-show], [0], [dnl
Default max sleep: 10000 us
])

dnl Check rounding
get_log_next_line_num
AT_CHECK([ovs-vsctl set open_vswitch . other_config:pmd-sleep-max="490"])
CHECK_DP_SLEEP_MAX([490], [enabled], [+$LINENUM])
AT_CHECK([ovs-appctl dpif-netdev/pmd-sleep-show], [0], [dnl
Default max sleep:  490 us
])

dnl Check rounding
get_log_next_line_num
AT_CHECK([ovs-vsctl set open_vswitch . other_config:pmd-sleep-max="499"])
CHECK_DP_SLEEP_MAX([499], [enabled], [+$LINENUM])
AT_CHECK([ovs-appctl dpif-netdev/pmd-sleep-show], [0], [dnl
Default max sleep:  499 us
])

OVS_VSWITCHD_STOP
AT_CLEANUP

AT_SETUP([PMD - revalidator modify overlapping flows])

OVS_VSWITCHD_START(
[add-port br0 p1 \
   -- set bridge br0 datapath-type=dummy \
   -- set interface p1 type=dummy-pmd \
   -- add-port br0 p2 \
   -- set interface p2 type=dummy-pmd
], [], [], [DUMMY_NUMA])

dnl Add one OpenFlow rule and generate a megaflow.
AT_CHECK([ovs-ofctl add-flow br0 'table=0,in_port=p1,ip,nw_dst=10.1.2.0/24,actions=p2'])
AT_CHECK([ovs-appctl netdev-dummy/receive p1 'ipv4(src=10.0.0.1,dst=10.1.2.2,proto=6),tcp(src=1,dst=2)'])

OVS_WAIT_UNTIL_EQUAL([ovs-appctl dpctl/dump-flows | sed 's/.*core: [[0-9]]*//'], [
recirc_id(0),in_port(1),packet_type(ns=0,id=0),eth_type(0x0800),ipv4(dst=10.1.2.2/255.255.255.0,frag=no), packets:0, bytes:0, used:never, actions:2])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 'ipv4(src=10.0.0.1,dst=10.1.2.2,proto=6),tcp(src=1,dst=2)'])
dnl Replace OpenFlow rules, trigger the revalidation.
AT_CHECK([echo 'table=0,in_port=p1,ip,nw_dst=10.1.0.0/16 actions=ct(commit)' | dnl
          ovs-ofctl --bundle replace-flows br0 -])
AT_CHECK([ovs-appctl revalidator/wait])

dnl Prevent flows from expiring.
AT_CHECK([ovs-appctl time/stop])

AT_CHECK([ovs-appctl netdev-dummy/receive p1 'ipv4(src=10.0.0.1,dst=10.1.0.2,proto=6),tcp(src=1,dst=2)'])
OVS_WAIT_UNTIL_EQUAL([ovs-appctl dpctl/dump-flows | sed 's/.*core: [[0-9]]*//' | strip_xout_keep_actions], [
recirc_id(0),in_port(1),packet_type(ns=0,id=0),eth_type(0x0800),ipv4(dst=10.1.0.2/255.255.0.0,frag=no), packets:0, bytes:0, used:never, actions:ct(commit)
recirc_id(0),in_port(1),packet_type(ns=0,id=0),eth_type(0x0800),ipv4(dst=10.1.2.2/255.255.255.0,frag=no), packets:0, bytes:0, used:0.0s, actions:ct(commit)])

dnl Send more 10.1.0.2 to make 10.1.0.0/16 tuple prepend 10.1.2.0/24 tuple in the pvector of subtables.
for i in $(seq 0 256); do
  AT_CHECK([ovs-appctl netdev-dummy/receive p1 'ipv4(src=10.0.0.1,dst=10.1.0.2,proto=6),tcp(src=1,dst=2)'])
done

dnl Warp time enough to trigger subtable optimization.
AT_CHECK([ovs-appctl time/warp 500 2000], [0], [ignore])

AT_CHECK([echo 'table=0,in_port=p1,ip,nw_dst=10.1.0.0/16 actions=p2' | dnl
          ovs-ofctl --bundle replace-flows br0 -])

AT_CHECK([ovs-appctl revalidator/wait])
AT_CHECK([ovs-appctl dpctl/dump-flows | sed 's/.*core: [[0-9]]*//' | strip_xout_keep_actions], [0], [
recirc_id(0),in_port(1),packet_type(ns=0,id=0),eth_type(0x0800),ipv4(dst=10.1.0.2/255.255.0.0,frag=no), packets:0, bytes:0, used:0.0s, actions:2
recirc_id(0),in_port(1),packet_type(ns=0,id=0),eth_type(0x0800),ipv4(dst=10.1.2.2/255.255.255.0,frag=no), packets:0, bytes:0, used:0.0s, actions:2
])

OVS_VSWITCHD_STOP
AT_CLEANUP
