m4_divert_push([PREPARE_TESTS])
[
# Strips out uninteresting parts of ovs-ofctl output, as well as parts
# that vary from one run to another.
ofctl_strip () {
    sed '
s/ (xid=0x[0-9a-fA-F]*)//
s/ duration=[0-9.]*s,//
s/ cookie=0x0,//
s/ table=0,//
s/ n_packets=0,//
s/ n_offload_packets=0,//
s/ n_bytes=0,//
s/ n_offload_bytes=0,//
s/ idle_age=[0-9]*,//
s/ hard_age=[0-9]*,//
s/dp_hash=0x[0-9a-f]*\//dp_hash=0x0\//
s/recirc_id=0x[0-9a-f]*,/recirc_id=0x0,/
s/[0-9][0-9][0-9][0-9]-[0-9][0-9]-[0-9][0-9]T[0-9][0-9]:[0-9][0-9]:[0-9][0-9]Z|//
s/dir\/[0-9]*\/br0.mgmt/dir\/XXXX\/br0.mgmt/
'
}

# Strips out byte counters from ovs-ofctl output
ofctl_strip_bytes () {
    sed 's/ n_bytes=[0-9]*,//'
}

# Filter (multiline) vconn debug messages from ovs-vswitchd.log.
# Use with vconn_sub() and ofctl_strip()
print_vconn_debug () { awk -F\| < ovs-vswitchd.log '
BEGIN { prt=0 }
/\|vconn\|DBG\|/ { sub(/[ \t]*$/, ""); print $3 "|" $4 "|" $5; prt=1; next }
$4 != "" { prt=0; next }
prt==1 { sub(/[ \t]*$/, ""); print $0 }
'
}

vconn_sub() {
    sed '
s/tcp:127.0.0.1:[0-9][0-9]*:/unix:/
s/unix#[0-9]*:/unix:/
'
}
]

# PARSE_LISTENING_PORT LOGFILE VARIABLE
#
# Parses the TCP or SSL/TLS port on which a server is listening from
# LOGFILE, given that the server was told to listen on a kernel-chosen
# port, and assigns the port number to shell VARIABLE.  You should
# specify the listening remote as ptcp:0:127.0.0.1 or
# pssl:0:127.0.0.1, or the equivalent with [::1] instead of 127.0.0.1.
#
# Here's an example of how to use this with ovsdb-server:
#
#    ovsdb-server --log-file --remote=ptcp:0:127.0.0.1 ...
#    PARSE_LISTENING_PORT([ovsdb-server.log], [TCP_PORT])
#    # Now $TCP_PORT holds the listening port.
m4_define([PARSE_LISTENING_PORT],
    [OVS_WAIT_UNTIL([$2=`sed -n 's/.*0:.*: listening on port \([[0-9]]*\)$/\1/p' "$1"` && test X != X"[$]$2"])])

start_daemon () {
    "$@" -vconsole:off --detach --no-chdir --pidfile --log-file
    pidfile="$OVS_RUNDIR"/$1.pid
    on_exit "test -e \"$pidfile\" && kill \`cat \"$pidfile\"\`"
}

# sim_add SANDBOX
#
# Starts a new simulated Open vSwitch instance named SANDBOX.  Files related to
# the instance, such as logs, databases, sockets, and pidfiles, are created in
# a subdirectory of the main test directory also named SANDBOX.  Afterward, the
# "as" command (see below) can be used to run Open vSwitch utilities in the
# context of the new sandbox.
#
# The new sandbox starts out without any bridges.  Use ovs-vsctl in the context
# of the new sandbox to create a bridge, e.g.:
#
#     sim_add hv0           # Create sandbox hv0.
#     as hv0                # Set hv0 as default sandbox.
#     ovs-vsctl add-br br0  # Add bridge br0 inside hv0.
#
# or:
#
#     sim_add hv0
#     as hv0 ovs-vsctl add-br br0
sims=
sim_add () {
   echo "adding simulator '$1'"

   sims="$sims $1"

   # Create sandbox.
   local d="$ovs_base"/$1
   mkdir "$d" || return 1
   ovs_setenv $1

   # Create database and start ovsdb-server.
   : > "$d"/.conf.db.~lock~
   as $1 ovsdb-tool create "$d"/conf.db "$abs_top_srcdir"/vswitchd/vswitch.ovsschema || return 1
   as $1 start_daemon ovsdb-server --remote=punix:"$d"/db.sock || return 1

   # Initialize database.
   as $1 ovs-vsctl --no-wait -- init || return 1

   # Start ovs-vswitchd
   as $1 start_daemon ovs-vswitchd --enable-dummy=system -vvconn -vofproto_dpif -vunixctl
}

# "as $1" sets the OVS_*DIR environment variables to point to $ovs_base/$1.
#
# "as $1 COMMAND..." sets those variables in a subshell and invokes COMMAND
# there.
as() {
    if test "X$2" != X; then
        (ovs_setenv $1; shift; "$@")
    else
        ovs_setenv $1
    fi
}

# Strips 'xid=0x1234' from ovs-ofctl output.
strip_xids () {
    sed 's/ (xid=0x[[0-9a-fA-F]]*)//'
}

# Changes all 'used:...' to say 'used:0.0', to make output easier to compare.
strip_used () {
    sed 's/used:[[0-9]]\.[[0-9]]*/used:0.0/'
}

# Removes all 'duration=...' to make output easier to compare.
strip_duration () {
    sed 's/duration=[[0-9.]]*s,//'
}

# Strips 'ufid:...' from output, to make it easier to compare.
# (ufids are random.)
strip_ufid () {
    sed 's/mega_ufid:[[-0-9a-f]]* //
    s/ufid:[[-0-9a-f]]* //'
}

parse_ufid () {
    grep -o 'ufid:[[-0-9a-f]]*'
}

# Strips packets: and bytes: from output
strip_stats () {
    sed 's/packets:[[0-9]]*/packets:0/
    s/bytes:[[0-9]]*/bytes:0/'
}

# Strips key32 field from output.
strip_key32 () {
    sed 's/key32([[0-9 \/]]*),//'
}

# Strips packet-type from output.
strip_ptype () {
    sed 's/packet_type(ns=[[0-9]]*,id=[[0-9]]*),//'
}

# Strips bare eth from output.
strip_eth () {
    sed 's/eth(),//'
}

# Changes all 'recirc(...)' and 'recirc=...' to say 'recirc(<recirc_id>)' and
# 'recirc=<recirc_id>' respectively.  This should make output easier to
# compare.
strip_recirc() {
   sed 's/recirc_id([[x0-9a-f]]*)/recirc_id(<recirc>)/
        s/recirc_id=[[x0-9a-f]]*/recirc_id=<recirc>/
        s/recirc([[x0-9a-f]]*)/recirc(<recirc>)/'
}

# Strips dp_hash from output.
strip_dp_hash() {
    sed 's/dp_hash([[0-9a-fx/]]*),//'
}

m4_divert_pop([PREPARE_TESTS])

m4_define([TESTABLE_LOG], [-vPATTERN:ANY:'%c|%p|%m'])

# _OVS_VSWITCHD_START([vswitchd-aux-args] [dbinit-aux-args])
#
# Creates an empty database and starts ovsdb-server.
# Starts ovs-vswitchd, with additional arguments 'vswitchd-aux-args'.
# 'dbinit-aux-args' are passed as additional commands to 'ovs-vsctl init'
# before starting ovs-vswitchd.
#
m4_define([_OVS_VSWITCHD_START],
  [dnl Create database.
   touch .conf.db.~lock~
   AT_CHECK([ovsdb-tool create conf.db $abs_top_srcdir/vswitchd/vswitch.ovsschema])

   dnl Start ovsdb-server.
   AT_CHECK([ovsdb-server --detach --no-chdir --pidfile --log-file --remote=punix:$OVS_RUNDIR/db.sock], [0], [], [stderr])
   on_exit "kill `cat ovsdb-server.pid`"
   AT_CHECK([[sed < stderr '
/vlog|INFO|opened log file/d
/ovsdb_server|INFO|ovsdb-server (Open vSwitch)/d']])
   AT_CAPTURE_FILE([ovsdb-server.log])

   dnl Initialize database.
   AT_CHECK([ovs-vsctl --no-wait init $2])

   dnl Start ovs-vswitchd.
   AT_CHECK([ovs-vswitchd $1 --detach --no-chdir --pidfile --log-file -vvconn -vofproto_dpif -vunixctl], [0], [], [stderr])
   AT_CAPTURE_FILE([ovs-vswitchd.log])
   on_exit "kill_ovs_vswitchd `cat ovs-vswitchd.pid`"
   AT_CHECK([[sed < stderr '
/ovs_numa|INFO|Discovered /d
/odp_execute_impl|INFO|Action implementation /d
/vlog|INFO|opened log file/d
/vswitchd|INFO|ovs-vswitchd (Open vSwitch)/d
/reconnect|INFO|/d
/dpif_netlink|INFO|Generic Netlink family .ovs_datapath. does not exist/d
/ofproto|INFO|using datapath ID/d
/netdev_linux|INFO|.*device has unknown hardware address family/d
/ofproto|INFO|datapath ID changed to fedcba9876543210/d
/dpdk|INFO|DPDK Disabled - Use other_config:dpdk-init to enable/d
/netlink_socket|INFO|netlink: could not enable listening to all nsid/d
/netdev_offload|INFO|netdev: Flow API Enabled/d
/probe tc:/d
/setting extended ack support failed/d
/tc: Using policy/d']])
])

# OVS_VSWITCHD_START([vsctl-args], [vsctl-output], [=override],
#                    [vswitchd-aux-args])
#
# Creates a database and starts ovsdb-server, starts ovs-vswitchd
# connected to that database, calls ovs-vsctl to create a bridge named
# br0 with predictable settings, passing 'vsctl-args' as additional
# commands to ovs-vsctl.  If 'vsctl-args' causes ovs-vsctl to provide
# output (e.g. because it includes "create" commands) then 'vsctl-output'
# specifies the expected output after filtering through uuidfilt.
#
# If a test needs to use "system" devices (as dummies), then specify
# =override (literally) as the third argument.  Otherwise, system devices
# won't work at all (which makes sense because tests should not access a
# system's real Ethernet devices).
#
# 'vswitchd-aux-args' provides a way to pass extra command line arguments
# to ovs-vswitchd
m4_define([OVS_VSWITCHD_START],
  [_OVS_VSWITCHD_START([--enable-dummy$3 --disable-system --disable-system-route $4])
   AT_CHECK([add_of_br 0 $1 m4_if([$2], [], [], [| uuidfilt])], [0], [$2])
])

# check_logs scans through all *.log files (except '*.log' and testsuite.log)
# and reports all WARN, ERR, EMER log entries.  User can add custom sed filters
# in $1.
m4_divert_push([PREPARE_TESTS])
check_logs () {
    local logs
    for log in *.log; do
        case ${log} in # (
            '*.log'|testsuite.log) ;; # (
            *) logs="${logs} ${log}" ;;
        esac
    done

    # We most notably ignore 'Broken pipe' warnings.  These often and
    # intermittently appear in ovsdb-server.log, because *ctl commands
    # (e.g. ovs-vsctl) exit right after committing a change to the
    # database.  However, in reaction, some daemon may immediately update the
    # database, and this later update may cause database sending update back to
    # *ctl command if *ctl has not exited yet.  If *ctl command exits before
    # the database calls send, the send fails with 'Broken pipe' or
    # 'not connected' depending on system.  Also removes all 'connection reset'
    # warning logs for similar reasons (EPIPE, ENOTCONN or ECONNRESET can be
    # returned on a send depending on whether the peer had unconsumed data
    # when it closed the socket).
    #
    # We also ignore "Dropped # log messages..." messages.  Otherwise, even if
    # we ignore the messages that were rate-limited, we can end up failing just
    # because of the announcement that rate-limiting happened (and in a racy,
    # timing-dependent way, too).
    #
    # We also ignore the "Spent an unreasonably long XXms dumping flows" as
    # they can appear when large time/warps are used during tests.
    sed -n "$1
/reset by peer/d
/Broken pipe/d
/is not connected/d
/timeval.*Unreasonably long [[0-9]]*ms poll interval/d
/timeval.*faults: [[0-9]]* minor, [[0-9]]* major/d
/timeval.*disk: [[0-9]]* reads, [[0-9]]* writes/d
/timeval.*context switches: [[0-9]]* voluntary, [[0-9]]* involuntary/d
/ovs_rcu.*blocked [[0-9]]* ms waiting for .* to quiesce/d
/Dropped [[0-9]]* log messages/d
/setting extended ack support failed/d
/ETHTOOL_GSSET_INFO/d
/Spent an unreasonably long .*ms dumping flows/d
/|WARN|/p
/|ERR|/p
/|EMER|/p" ${logs}
}

# Gets the last line number in ovs-vswitchd.log +1. This can be used to
# help ensure that an output in the log is newly written as the result of
# a test command and it is not just matching an earlier log line.
get_log_next_line_num () {
    LINENUM=$(($(cat ovs-vswitchd.log | wc -l | tr -d [[:blank:]])+1))
}

# add_of_br BRNUM [ARG...]
add_of_br () {
    local brnum=$1; shift
    local br=br$brnum
    local dpid=fedcba987654321$brnum
    local mac=aa:55:aa:55:00:0$brnum
    ovs-vsctl \
        -- add-br $br \
        -- set bridge $br datapath-type=dummy \
                          fail-mode=secure \
                          other-config:datapath-id=$dpid \
                          other-config:hwaddr=$mac \
                          protocols="[[OpenFlow10,OpenFlow11,OpenFlow12,\
                                       OpenFlow13,OpenFlow14,OpenFlow15]]" \
        -- "$@"
}

# add_of_ports__ PORT_TYPE [--pcap] BRIDGE PNUM...
#
# Creates PORT_TYPE interfaces in BRIDGE named pPNUM, OpenFlow port number
# PNUM, and datapath port number PNUM (the latter is a consequence of
# the dummy implementation, which tries to assign datapath port
# numbers based on port names).
#
# If --pcap is supplied then packets received from the interface will
# be written to $port-rx.pcap and those sent to it to $port-tx.pcap.
add_of_ports__ () {
    local args
    local pcap=false
    local ptype=$1
    shift
    if test "$1" = --pcap; then
        pcap=:
    shift
    fi
    local br=$1; shift
    for pnum; do
        AS_VAR_APPEND([args], [" -- add-port $br p$pnum -- set Interface p$pnum type=$ptype ofport_request=$pnum"])
    if $pcap; then
        AS_VAR_APPEND([args], [" -- set Interface p$pnum options:rxq_pcap=p$pnum-rx.pcap options:tx_pcap=p$pnum-tx.pcap"])
    fi
    done
    echo ovs-vsctl $args
    ovs-vsctl $args
}

# add_of_ports [--pcap] BRIDGE PNUM...
#
add_of_ports () {
    add_of_ports__ dummy $@
}

# add_pmd_of_ports [--pcap] BRIDGE PNUM...
#
add_pmd_of_ports () {
    add_of_ports__ dummy-pmd $@
}

m4_divert_pop([PREPARE_TESTS])

# OVS_VSWITCHD_STOP([ALLOWLIST])
#
# Gracefully stops ovs-vswitchd and ovsdb-server, checking their log files
# for messages with severity WARN or higher and signaling an error if any
# is present.  The optional ALLOWLIST may contain shell-quoted "sed"
# commands to delete any warnings that are actually expected, e.g.:
#
#   OVS_VSWITCHD_STOP(["/expected error/d"])
m4_define([OVS_VSWITCHD_STOP],
  [AT_CHECK([check_logs $1])
   OVS_APP_EXIT_AND_WAIT([ovs-vswitchd])
   OVS_APP_EXIT_AND_WAIT([ovsdb-server])])

m4_define([OVS_VSWITCHD_DISABLE_TUNNEL_PUSH_POP],
  [AT_CHECK([ovs-appctl dpif/set-dp-features br0 tnl_push_pop false], [0])
])

# WAIT_FOR_DUMMY_PORTS(NETDEV_DUMMY_PORT[, NETDEV_DUMMY_PORT...])
#
# Wait until the netdev dummy ports are connected to each other
m4_define([WAIT_FOR_DUMMY_PORTS], \
  [m4_foreach([dummy_port], [$@],
      [  \
         OVS_WAIT_WHILE([ovs-appctl netdev-dummy/conn-state dummy_port \
                  | grep 'unknown\|disconnected'])])])


