# Sum of option lengths would overflow RDLEN
#
# OPT RDATA, RDLEN=14 (0x000e)
000e
# Pseudo RR 1 (code=3, len=3)
00 03 00 03 00 01 02
# Pseudo RR 2 (code=4, len=65535 overflows RDLEN)
00 04 ff ff 00 01 02
# Rest of option data is omitted...
